**Dam Safety Inspection**

**Stedman Lake Dam (Stokes County, NC)**

* [← Go Back](https://data.hollandsentinel.com/dam/north-carolina/stokes-county/stedman-lake-dam/nc00341/)

Dam Detail

|  |  |  |
| --- | --- | --- |
| Hazard Potential Classification | | Low |
| Condition Assessment | | Satisfactory |
| EAP Prepared | | No |
| Dam Name | Stedman Lake Dam |
| Other Name | Issac Walton League Dam |
| NID ID | NC00341 |
| Federal ID | NC00341 |
| Owner Names | Ashley Montague |
| Owner Types | Private |
| Primary Owner Type | Private |
| State or Federal Agency ID | STOKE-033 |
| State Regulated Dam | Yes |
| State Jurisdictional Dam | Yes |
| State Regulatory Agency | NCDEQ, DEMLR, Dam Safety Program |
| State Permitting Authority | Yes |
| State Inspection Authority | Yes |
| State Enforcement Authority | Yes |
| Source Agency | North Carolina |
| County Equivalent | Stokes |
| State | North Carolina |
| Nearest City | Danbury |
| Distance to Nearest City (Miles) | 3 |
| River or Stream Name | Dan River |
| Congressional District | North Carolina, Congressional District 05 |
| Website URL | <https://damsafety.org/north-carolina> |

|  |  |
| --- | --- |
| Primary Purpose | Recreation |
| Purposes | Recreation |
| Primary Dam Type | Concrete |
| Dam Types | Concrete;Arch |
| Hydraulic Height (Ft) | 28 |
| Structural Height (Ft) | 30 |
| NID Height (Ft) | 30 |
| NID Height Category | 25-50 feet |
| Dam Length (Ft) | 140 |
| Year Completed | 1919 |
| Year Completed Category | 1910-1919 |
| NID Storage (Acre-Ft) | 96.0 |
| Max Storage (Acre-Ft) | 96.0 |
| Normal Storage (Acre-Ft) | 90.0 |
| Surface Area (Acres) | 8.0 |
| Drainage Area (Sq Miles) | 877.00 |
| Max Discharge (Cubic Ft/Second) | 99 |

* [← Go Back](https://data.hollandsentinel.com/dam/north-carolina/stokes-county/stedman-lake-dam/nc00341/)

Map

[DamsCounty](https://data.hollandsentinel.com/dam/north-carolina/stokes-county/stedman-lake-dam/nc00341/)